Alexander Culbert

12-14-2018

BME 590L

Current Draw Testing

At rest: 5.57 mA

At low: 9.54 mA

At medium: 12.41 mA

At high: 17.93 mA

Flashing 6.81, 17.93 mA alternating